# Summary of Algorithms used by PlanetarySystemStacker

This document is a algorithmic guide through the open-source software “PlanetarySystemStacker”. It explains all the steps performed in stacking a video file or batch of single images. For every step it lists the data structures and configuration parameters (*cursive*) involved in the operation and states where in the code the step is performed.

|  |  |  |
| --- | --- | --- |
| **Description of algorithmic step** | **Data strcuture(s) involved** | **Module.Class.Method or Module.Function**  **in Python source code** |
| **GUI control** |  |  |
| PlanetarySystemStacker comes with a GUI using the QT5 widget toolkit. The GUI is started with the main program in module “planetary\_system\_stacker.py”.  The GUI starts a separate “workflow” thread which does all computations, especially those in batch mode.  Individual processing phases of the workflow are triggered by the GUI using QT signals associated with slots in the Workflow object. The signals are emitted in method “work\_next\_task”.  The processing steps are the same as described below for the version using a main program without GUI. That version is mostly used for debugging purposes. The processing details, therefore, in the following are described for the main program case only. |  | planetary\_system\_stacker. \_\_main\_\_  planetary\_system\_stacker. PlanetarySystemStacker.init  workflow.Workflow  planetary\_system\_stacker. PlanetarySystemStacker. work\_next\_task |
| **Main control program (for debugging)** |  |  |
| All parameters controlling the program are set in the configuration object. Eventually these values are to be set by the GUI and maintained between executions in a configuration file. |  | configuration.Configuration |
| Set the names of files to process. This can either be the names of video files (type .avi) or names of directories containing image files (type .tiff). In the latter case all files of one directory are taken as input for a single stacking operation. If those images differ in shape, an error is raised.  If multiple video files or multiple directories are specified, multiple stacking operations are performed in batch mode in succession.  The workflow for the entire stacking process for a video file or image directory is controlled by the “workflow” function. | input\_names  input\_type = “video” or “image” | main\_program.\_\_main\_\_  main\_program.workflow |
| Optional: Select a “region of interest” (ROI) in the form (y\_low, y\_high, x\_low, x\_high). If set to “None”, the full frames are used | roi | main\_program.\_\_main\_\_ |
| Optional: Select that input images should be converted to grayscale before processing. If set to “None”, color images are processed as three-channel RGB. | convert\_to\_grayscale = True or False | main\_program.\_\_main\_\_ |
| For performance measurements, code sections can be timed. If the same section is executed several times, counters can be incremented. A timer object is created at start of execution. Individual counters can be added later. In the end, a table with the accumulated times of all counters can be printed. | my\_timer | timer.timer |
| **Read frames and create derived images** |  |  |
| PlanetarySystemStacker provides several buffering levels of data which are used more than once during a stacking job. For level 0, no data are buffered. Images are read from the input file when needed, and derived versions are re-computed. For level 4, frames are read only once, and all derived image versions are kept in memory.  The program uses four versions of the image data:   * The original image data, either read from a single .avi file, or from a directory with image files. The shape of a single frame is (pixels in y, pixels in x [, 3 in case of color]). * 2D monochrome image (if the original frames were monochrome, this is just a pointer to the original frame) * “Blurred” version of the monochrome image. It is computed by applying a Gaussian filter to the monochrome image. The width of the Gaussian is an input parameter. * Laplacian of the Gaussian   Access to the four image versions is via methods of class “Frame”. Depending on whether the data are buffered or not, a pointer to the object in memory is returned, or the image is read from the input file and/or computed by applying the appropriate filter.  The blurred image versions are used later in shift computations. This helps avoiding spurious local minima caused by pixel noise.  The Laplacians are used for ranking image quality. This happens in two locations: First in ranking the overall frame quality for constructing the mean frame, and then when the frame quality in local areas around alignment points is computed in the stacking process. | parameter: *global\_parameters\_buffering\_ level*  frames\_original  frames\_monochrome  frames\_monochrome\_blurred  frames\_monochrome\_blurred\_ laplacian  parameter: *frames\_gauss\_width* | frames.Frames.init  frames.Frames.frames  frames.Frames.frames\_mono  frames.Frames.frames\_mono\_ blurred  frames.Frames.frames\_mono\_ blurred\_laplacian |
| **Global frame ranking** |  |  |
| Next all frames are ordered by their overall image quality. This is done by computing the amount of structure in the (“blurred” monochrome) images. Three methods can be selected for ranking, using one of the following expressions (greater value is better) on the local luminance :   * “xy gradient”: * “Laplace”: ) * “Sobel”:   with and being the horizontal / vertical Sobel operators.   The values are normalized, so that the value for the best frame is 1.0. The index of the frame with the highest rank is computed. This frame is used as the reference for the computation of global frame shifts.  A stride value can be specified. If set to a value > 1, the images are down-sampled by this value before computing the score. In typical video files setting a value of 2 usually gives a good ranking and saves compute time.  Usually the method “Laplace” is to be preferred. | frame\_ranks  frame\_ranks\_max\_index  parameters:  *rank\_frames\_method*  *rank\_frames\_pixel\_stride* | rank\_frames.RankFrames. frame\_score  methods:   * local\_contrast * local\_contrast\_laplace * local\_contrast\_sobel   in class  miscellaneous.Miscellaneous |
| **Global frame alignment** |  |  |
| Next all frames are aligned with each other. The frame with the highest rank is used as reference (see above). Two alignment modes are available: “Surface” and “Planet”.   * “Surface”: First find a rectangular patch with good structure as “alignment window”. The size of the patch is a fraction of the frame size, the scale factor being a configuration parameter. By setting a parameter “align\_frames\_border\_width” the window can be kept away from the frame borders. This way, the window does not have to be moved as often when the object is drifting between frames.  For all potential alignment patches in the frame the merit function  min(,  is executed. This way the patch is found where good vertical and horizontal structures are present. In order to ignore contributions by noise in dark areas, a brightness threshold is included. An ordered list of alignment patches with decreasing merit function is computed. Frame alignment (see below) is tried using the patch with the highest score. If it fails for some frame, the process is repeated using the next patch, and so on, until the alignment succeeds for all frames or there are no patches left.  Next all frames are compared with the reference frame at this patch, and the relative shift is computed. Three methods are available for this search: - “Translation” (not recommended): Cross-correlation  - “RadialSearch” (stable but expensive): Search all positions for a local minimum of the expression given below, spiraling out from zero shift. - “SteepestDescent” (recommended, and used exclusively by the GUI version): Same as “RadialSearch”, but not all positions around zero shift are evaluated, but only those in the direction of the steepest descent of the evaluation function. More precisely:  Starting with shift values [dy\_min, dx\_min] = [0, 0], the shifted alignment window in the current frame is compared with the reference frame window. For every search position, the match quality is computed with   A “sampling stride” parameter can be selected. In this case the summation indices are incremented using this stride (to save compute time).  First, for all positions with distance 1 in y or x the match quality is computed. If the minimal value is smaller than the best value so far, the corresponding position is taken as a new start point.   For this new start point, again all positions with distance 1 are tested in search for a better minimum. The search ends when no improvement is found, or the maximum search width (parameter) is reached. In the latter case, the search is regarded as unsuccessful.  Consecutive frames tend to have similar shifts. Therefore, the optimum found for one frame is taken as start value for the next one. The current shift is kept in the cumulative shifts [dy\_min\_cum, dx\_min\_cum].  All frame shifts are measured relative to the reference frame. To make it easier for the search algorithm described above, the computation starts for the frame captured just before the reference frame, and going backwards until the first frame is reached. In a second loop, the remaining frames are treated starting with the frame just after the reference frame and going to the end of the video. This way, the search always starts with a good approximation.  If the object drift is too large, the alignment window can hit the frame border. Before that happens, the window is shifted by half the border width away from the border. * “Planet”: Only applicable if the object is surrounded by black space in all directions. In this case alignment is much easier. For each frame the “center of gravity” of the brightness distribution is computed. The differences in y and x give the relative shift. | Parameters:  *align\_frames\_mode*  *align\_frames\_rectangle\_ scale\_factor*  *align\_frames\_rectangle\_ black\_threshold*  *align\_frames\_search\_width*  *align\_frames\_border\_width*  *align\_frames\_sampling\_stride*  *align\_frames\_ average\_frame\_percent*  alignment\_rect\_qualities  frame\_shifts    [dy\_min\_cum, dx\_min\_cum] | miscellaneous.Miscellaneous. quality\_measure\_alternative  align\_frames.AlignFrames. compute\_alignment\_rect  align\_frames.AlignFrames. select\_alignment\_rect  align\_frames. AlignFrames.align\_frames  miscellaneous.Miscellaneous. translation  miscellaneous.Miscellaneous. search\_local\_match  miscellaneous.Miscellaneous. search\_local\_match\_gradient |
| After aligning all frames, the pixel bounds of the intersection of all frames are computed: intersection\_shape[y, x][low, high] | intersection\_shape |  |
| **Mean frame computation** |  |  |
| Next, the average frame is computed by averaging the best frames, taking into account their relative global shifts. At this point no local warp effects can be corrected for. The percentage of the total number of frames is chosen via a parameter.  From now on, pixel indexing of new image objects uses the shape of the average frame, given by the index bounds in the structure “intersection\_shape”. The original frames, however, are not copied, so they keep their original indexing. The global shifts between the image frames and the new reduced-size images are stored in lists “dy” and “dx” in the “align\_frames” object. | average\_frame  Parameter: *align\_frames\_average\_frame\_ percent*  dy / dx | align\_frames.AlignFrames. average\_frame |
| If a “region of interest” was selected, the intersection is reduced to this size and position in the frame. A new mean frame is computed with the new intersection shape. |  | align\_frames.AlignFrames. set\_roi |
| **Alignment point creation** |  |  |
| Next, the alignment points (APs) for the “multi-point alignment” are defined. The methods are contained in class “alignment\_points”. All alignment points are organized in a linear list. Each entry is a dictionary containing all information on a single point. The main variables in that dictionary are:   * y, x pixel coordinates of center * Lower and upper index bounds in y and x of the so-called “alignment box”. This is the area used for measuring the local (warp) shift against the mean frame. * Lower and upper index bounds in y and x of the so-called “alignment patch”. The patch is somewhat larger than the box. It is the area used for stacking around this AP. * The “reference box” with the section of the average frame at the location of the alignment box. * The stacking buffer where frame contributions are accumulated during stacking for this alignment patch.   Usually, first a grid of alignment points is created automatically, using the method “create\_ap\_grid”. The AP distance in y and x is specified with the “step\_size” parameter. Additional points can be added or removed individually (“new\_alignment\_point”, “remove\_alignment\_points”). The following example shows the result of an automatic AP creation. The picture is created by method “show\_alignment\_points”. Red crosses show the (real) alignment points. White and green quadrats are the alignment boxes and patches around the APs, respectively.  D:\SW-Development\Python\PlanetarySystemStacker\Examples\Saturn\sat_c11_ser_F0001-1731.avi.aps_copy.jpg  The automatic AP creation produces a staggered grid of points. In rows where the first and last points are farther away from the frame boundary, alignment patches are extended up to the frame boundary (in order to avoid holes).  In AP grid creation, APs are put on the AP list only if they satisfy several conditions:   * The alignment box must contain pixels brighter or equal to a given threshold (brightness condition). * The difference between the brightest and dimmest pixels in the alignment box must be greater or equal to a second threshold (contrast condition). * A “structure” value representing the amount of local structure in the alignment box must exceed a third threshold (structure threshold). The values are normalized such that it is 1. for the AP with maximum structure. | alignment\_points  Parameters:  *alignment\_points\_half\_box\_ width*  *alignment\_points\_half\_patch\_ width*  *alignment\_points\_step\_size*  *alignment\_points\_brightness\_ threshold*  *alignment\_points\_contrast\_ threshold*  *alignment\_points\_structure\_ threshold* | alignment\_points. AlignmentPoints. create\_ap\_grid  alignment\_points. AlignmentPoints. new\_alignment\_point  alignment\_points. AlignmentPoints. remove\_alignment\_points  alignment\_points. AlignmentPoints. find\_alignment\_points  alignment\_points. AlignmentPoints. find\_neighbor  alignment\_points. AlignmentPoints. show\_alignment\_points |
| Special attention is given to APs in dark areas close to the moon or planet. If the AP satisfies the structure and brightness condition, the object must fill at least part of the alignment box. To find APs where this part is too small, the fraction of pixels brighter than the brightness threshold is computed. If it is smaller than parameter “dim\_fraction\_threshold”, the AP is moved towards the object. To this end, the “center of gravity” of the bright pixels inside the alignment box is computed, and the AP center is moved to this point. | Parameter:  *alignment\_points\_dim\_fraction\_ threshold* |  |
| Finally, for each AP the amount of structure in the AP box is computed using the expression  ,  If the sharpness value is below the given threshold, the alignment point is added to the list of failed APs. | Parameter:  *alignment\_points\_structure\_ threshold* | miscellaneous.Miscellaneous. quality\_measure |
| **Ranking frames at alignment points** |  |  |
| After all APs have been set, for each frame and each AP the image quality is computed, based on the alignment box around the AP. This is a very compute intensive operation. For computing the local frame qualities, as above three methods can be chosen from (by selecting the “rank\_method” parameter:   * “xy gradient” * “Laplace” * “Sobel”   For their definition, see above. The recommended choice is “Laplace”. It is used by the GUI version of PSS.  As with frame ranking, a stride parameter can be set for down-sampling. If the “Laplace” method had been chosen to rank the frames, and now again “Laplace” is chosen for AP ranking, sampled-down Laplacians were stored for re-use. In this case the parameter “alignment\_point\_pixel\_stride” is ignored, and the old parameter “rank\_frames\_pixel\_stride” is re-used instead (because the Laplacians were computed with this stride).  The qualities are stored for all frames in a list. The list is stored in the AP dictionary as “alignment\_point[‘frame\_qualities’]. A list of the best frame indices (up to the specified percentage of frames to be stacked) is computed and stored in the AP dictionary as “alignment\_point[‘best\_frame\_indices’]. Note that these lists in general are different at different APs because of local seeing.  To make the association of APs and best frames also accessible from the frame side, the APs are appended to the list of “used alignment points” of their corresponding frame objects. These lists are used in stacking below. | alignment\_point[ ‘frame\_qualities’]  alignment\_point[ ‘best\_frame\_indices’]  Parameters:  *alignment\_points\_rank\_ method*  *alignment\_points\_pixel\_stride*  *alignment\_points\_frame\_ percent*  frames.used\_alignment\_points | alignment\_points. AlignmentPoints. compute\_frame\_qualities |
| **Frame stacking** |  |  |
| In preparation of frame stacking, method “prepare\_for\_stack\_blending” is executed. It computes all auxiliary arrays and variables, so that in the remaining computations each video frame has to be loaded only once.  First, by looping over all APs, for every pixel the number of frames which in stacking will contribute to this pixel is computed (array “number\_single\_frame\_contributions”). If all pixels are covered, no background image is needed.  Next, for every AP an array with the size of the AP patch is computed. It is filled with “weights” between 0 and 1. Weights are 0 outside the patch rim and increase linearly to 1 on the box rim. Within the box the weight is set constant to 1. The helper function “one\_dim\_weight” computes the ramping from zero to one and back to zero across a 1D line through the patch. Array “sum\_single\_frame\_weights” accumulates the contributions from all APs. This array is used later for buffer normalization.  The variable “number\_stacking\_holes” contains the number of zero entries in array “number\_single\_frame\_contributions”, i.e. the number of pixels where the background image is needed in stacking. “fraction\_stacking\_holes” is the fraction of those pixels as compared to the entire image.  If “number\_stacking\_holes” is zero, no background image is needed in stacking. In this case everything is set for stacking.  If it is greater than zero, the stacked image contains holes, so it has to be blended with a background image. The background is computed as the average of the best frames. Only global shifts are applied, no warping. This image must be blended gradually with the stacked image. This is done using a mask array which is set to:   * 0. at points not covered by a single AP patch (i.e. a hole). * 1. at points covered by more than one AP patch, and at points within the interior (AP box) of a single AP. * between 0. and 1. in the transition area between the holes and the AP boxes.   A smooth transition is achieved by applying a Gaussian blur to the mask. This creates two problems:   * Mask values can be smaller than 1. in the AP interior, so the background must be available there, too. This is taken care of by recomputing the pixel positions where the background must be available after blurring the mask. * Maks values can be greater than 0. in the holes where no AP contribution is available. This latter problem is solved by resetting values back to 0. there.   Based on “fraction\_stacking\_holes” it is decided if it is worthwhile to compute a complete background image. If the fraction is small (relative to the parameter “stack\_frames\_background\_fraction”, the background is only computed in patches around pixels where it is needed.  A list “backgroune\_patches” of dictionaries is constructed. For each patch where the background image is to be computed during stacking, it specifies the bounds in y and x. | stack\_frames.number\_single\_ frame\_contributions  alignment\_point['weights\_yx']  sum\_single\_frame\_weights  number\_stacking\_holes,  fraction\_stacking\_holes  mask, mask\_intermediate  Parameter:  stack\_frames\_gauss\_width  Parameter:  stack\_frames\_background\_ fraction  background\_patches | stack\_frames. prepare\_for\_stack\_blending |
| Frame stacking proceeds in a loop over all frames. For each frame there is a loop over all alignment points for which it was decided before that this frame is to be used (see “Rank frames at alignment points”). | Frames.used\_alignment\_points | stack\_frames. StackFrames.stack\_frames |
| First, the local shift of the frame at the AP is computed relative to the mean frame. Similar as with the computation of global frame shifts, four methods can be chosen from (see Section “Global frame alignment” for details):   * “Subpixel” * “CrossCorrelation” * “RadialSearch” * “SteepestDescent”   The recommended version is “SteepestDescent”. It is most stable, reasonably fast and reliable.  As in Section “global frame alignment”, a parameter “sampling\_stride” can be set > 1 to speed up the process. In this case the optimal position of the local shift is still determined with 1 pixel accuracy, but the summation in the merit function only includes a coarser subset of pixels. A good match should still lead to a minimum of the merit function at the right place, in particular since the merit function is evaluated on the blurred monochrome images. | *shift\_pixel*  Parameters:  *alignment\_points\_method*  *alignment\_points\_sampling\_stride* | alignment\_points. AlignmentPoints. compute\_shift\_alignment\_point |
| Next, the total shift at the AP is computed as the sum of the global frame shift and the local warp shift “shift\_pixel”. Using these shift values, function “remap\_rigid” shifts the AP patch around the AP in the current frame and adds it to the AP’s stacking buffer. Here for the first time the original (color) frames are used, and not the blurred monochrome versions which had been the basis for all quality analyses and shift computations. | [total\_shift\_y, total\_shift\_x]  alignment\_point[ ‘stacking buffer’] | stack\_frames. StackFrames.remap\_rigid |
| Within the same loop over all frames, the (partial) background image is computed. Therefore, each frame has to be loaded only once. | averaged\_background |  |
| **Merging alignment patches** |  |  |
| So far stacking was performed locally on the AP patches. Now those patches are blended into the global “stacked\_image\_buffer”. This is done by method “merge\_alignment\_point\_buffers”.  It is crucial at this step to avoid sharp transitions between patches. After all, they have been rigidly shifted, most likely using different shift values. Therefore, overlapping patches must be blended with each other. The difficulty is, however, that the program so far has no notion of AP neighborhood. This problem is solved by multiplying the AP patches with weight functions which smoothly go to zero on the patch rim.  In the next step, the global image buffer (“stacked\_image\_buffer”) is divided pixel-wise by the “sum\_single\_frame\_weights” buffer. As a result of this “normalization” the overall brightness values of the “stacked\_image\_buffer” correspond to the mean brightness of the stacked images. In particular, neighboring patches are blended with each other with the same overall weight at every pixel. This is true, however, only for pixels where at least one AP patch has contributed. There might be holes in between.  If there are holes between the AP patches (i.e. “fraction\_stacking\_holes” is greater than 0), they are filled by blending the image “stacked\_image\_buffer” with the array “averaged\_background”. This array was computed by averaging those frames with the highest overall quality, only taking into account their global relative shifts (no local warping). | stacked\_image\_buffer  Alignment\_point[‘weights\_yx’]  sum\_single\_frame\_weights  fraction\_stacking\_holes | stack\_frames.StackFrames. merge\_alignment\_point\_buffers  stack\_frames.StackFrames. one\_dim\_weight |
| **Saving the final image** |  |  |
| Finally, the “stacked\_image\_buffer” is written to a file. At this point only 16bit Tiff is supported. | stacked\_image\_buffer | frames.Frames.save\_image |